{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["预算"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"预算","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"merged":[[0,1,0,6],[1,1,4,1],[5,1,9,1],[10,3,10,6],[11,1,11,6]],"flags":["formulas_cached_only"]}
[null,"公厕维修报价单"]
[null,"建安大道公厕","项目名称","单位","数量","施工工艺","报价"]
[null,null,"屋顶防水","平方",172,"去除鼓起的旧卷材，清理干净，刷防水胶，屋顶全铺法，采用热熔法，喷枪烤溶卷材底面，趁热压实卷材全部包围阴阳角及围墙\n"]
[null,null,"室内墙体批墙粉刷","平方",120,"搭建2层脚手架，人工抹腻子找平打磨光滑用乳胶漆刷2-3边\n"]
[null,null,"室外墙体批墙粉刷与造型修复","项",1,"采用高空作业车或搭建2层脚手架人工抹腻子找平打磨光滑用腻子修复造型；刷室外防水乳胶漆\n"]
[null,"七一路公厕","屋顶防水","平方",72,"去除鼓起的旧卷材，清理干净，刷防水胶，屋顶全铺法，采用热熔法，喷枪烤溶卷材底面，趁热压实卷材全部包围阴阳角及围墙\n\n"]
[null,null,"室内墙体批墙粉刷（上下2层）","平方",140,"搭建2层脚手架，人工去铲除鼓起面，抹腻子找平打磨光滑用乳胶漆刷2-3边"]
[null,null,"室外墙体批墙粉刷与造型修复","项",1,"采用高空作业车或者搭3到4层脚手架人工抹腻子找平打磨光滑用腻子修复造型；刷室外防水乳胶漆2到3遍 顶部造型瓦清洁 外墙字体加固"]
[null,null,"防盗窗拆除打磨喷漆与安装","个",21,"高空作业车拆下防盗窗，在喷漆房内除锈打磨喷一遍防锈漆，再喷2-3遍黑色金属漆，用高空作业车装回\n\n\n"]
[null,null,"房顶外围灯拆除","项",1,"用高空作业车人工拆除"]
[null,"合计","                      ¥.","报价公司："]
[null,"注：可能会有部分误差，请各位意向施工方前往查看后报最终价格"]